Bugs fixed:

1. Fixed the problems of input source flashing on the MVR display and output blurring during debugging and switching between PVW and PGM.
2. Fixed the color cast problem of LCD (v2.0.0.0).
3. Fixed the problem that the1280×1344 resolution set during screen configuration changes automatically to 1536×1344 in the 1×3 splicer mode.

Applicable hardware version: C/D/F

Supporting products:

V-Can: V3.3.0 or earlier

C1: V1.2.1.0 or earlier