J6 V2.2.0.0 STD Update Notes

1. New features

(1) Supports AUX function. The DVI\_OUT3 supports AUX output in Switcher mode.

(2) Supports BKG function in Splicer mode.

(3) Supports preset transition effect in Splicer mode.

(4) Supports the new SDI card of the J6.

(5) Supports the multiple control function of the C1.

(6) Supports up to 32 presets (10 presets supported earlier).

2. Bug fixes

(1) The BKG image blurs after the screen layout is changed.

(2) The screen flashes after the Black Out or Freeze command is sent by the J6 when it works with certain video processing devices.

(3) The Black Out effect controlled by the C1 or V-Can on control computer together with the J6 becomes invalid automatically when the Ethernet cable between the J6 and the C1 or the control computer is disconnected.

(4) The color cast problem occurs when the default color parameter values are changed.

(5) The SDI video sources from some cameras cannot be recognized.